For 1990-2009 cars

Because the problems in steering, suspension, and tires and wheels involve several systems, you must consider all of these systems whenever you diagnose a concern. In order to avoid diagnosing the wrong symptom, always road test the vehicle first. Proceed with the following preliminary tests, and correct any substandard conditions which you may find.

Inspect for the following conditions:

• | Wrong pressure and uneven tire wear

• | Loose connections or wear on joints, from the steering column to the steering gear

• | Loose or damaged parts on the front and on the rear suspension or on the steering gear

• | Out-of-round or out-of-balance tires, bent wheels, and loose or rough wheel bearings

• | Leaks in the power steering system. Inspect the power steering fluid level and inspect the accessory drive belt for proper condition and tension