For 1990-2009 cars

Caution: NEVER spray water on a hot heat exchanger. The resulting steam could cause personal injury.

Notice: The heat exchanger fins are necessary for good heat transfer. Do not brush the fins. This may cause damage to the fins, reducing heat transfer.

Important: Do not brush the radiator fins. The radiator fins are necessary for good heat transfer. Brushing damages the fins and reduces heat transfer.

Clean the front face of the radiator annually.

• | Clean the front face of the condenser.

• | Remove bugs, leaves, etc. by blowing compressed air through the radiator.

| Blow the air from the rear toward the front. If compressed air is not available a water hose can be used to force water through the radiator.

| Us only cool water with the engine not running.