For 1990-2009 cars

# DA6 AIR CONDITIONING COMPRESSOR TOOL MODIFICATION

#### VEHICLES AFFECTED: All Carlines

Kent-Moore special tool J-33013, Hub and Drive Plate Remover and Installer, which is an available tool may not properly fit the compressor shaft during Hub and Drive Plate Removal.

The tool should be reworked as shown in the figure below.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.