For 1990-2009 cars

## Automatic Transmission Components V6 VIN K

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Automatic Transmission (V6 VIN K) | Behind the engine | Antilock Brake System Component Views in ABS Traction Control | --
Cruise Control/Clutch Anticipate Switch (V6 VIN K ) | Mounted in the clutch pedal bracket | Cruise Control Component Views in Cruise Control | Cruise Control Connector End Views in Cruise Control
Cruise Control (Clutch) Switch (V8 VIN G Manual) | Mounted in the clutch pedal bracket | Harness Routing Views in Wiring Systems | Cruise Control Connector End Views in Cruise Control
Park Neutral Position Switch | Under the center console, on the base of the shift control lever | -- | Engine Electrical Connector End Views in Starting and Charging
Powertrain Control Module (PCM) (V6 VIN K) | On the right side of the engine compartment, rear of the wheelhouse | Harness Routing Views in Wiring Systems | --
Powertrain Control Module (PCM) (V8 VIN G) | On the right side of the engine compartment, rear of the wheelhouse | Engine Controls Component Views in Engine Controls 5.8L | --
Second Gear Start Switch (V6 VIN K) (Chevrolet) | In the center of the IP, above the HVAC control | Antilock Brake System Component Views in ABS Traction Control | --
Stop Lamp Switch | Mounted on the brake pedal bracket | Cruise Control Component Views in Cruise Control | --
Stop Lamp/TCC Switch (Automatic) | Mounted on the brake pedal bracket | -- | Lighting Systems Connector End Views in Lighting Systems
Underhood Electrical Center 2 | In the left front corner of the engine compartment | Engine Controls Component Views in Engine Controls 5.8L |
Vehicle Speed Sensor (Manual) | On the rear left side of the transmission | Antilock Brake System Component Views in ABS Traction Control | Engine Controls Connector End Views in Engine Controls
Vehicle Speed Sensor (Automatic) | On the rear right side of the transmission | Antilock Brake System Component Views in ABS Traction Control | Engine Controls Connector End Views in Engine Controls
C100 (10 cavities) | Engine to forward lamp harness, in the engine compartment, above the right wheelhouse | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C105 (8 cavities) | Engine to forward lamp harness, in the engine compartment, above the right wheelhouse | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200A (17 cavities) | Forward lamp to IP harness, between the left kick panel and the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200B (18 cavities) | Forward lamp to IP harness, between the left kick panel and the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200D (48 cavities) | Part of the IP harness, between the left kick panel and the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C210 (10 cavities) | IP to engine harness, under the right side of the IP, behind the knee bolster | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C220 (10 cavities) | IP to engine harness, under the right side of the IP, behind the knee bolster | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C270 (2 cavities) | IP harness of the cruise control harness, near the brake/clutch pedal bracket | Harness Routing Views in Wiring Systems | --
G110 (V8 VIN G) | Attached to the rear of the left cylinder head | Harness Routing Views in Wiring Systems | --
G110 (V6 VIN K) | In the front of the engine, bolted to the pulley above the A/C clutch connector | Harness Routing Views in Wiring Systems | --
P100 | Left side in the dash panel, engine to the passenger compartment | Harness Routing Views in Wiring Systems | --
P110 | Right side in the dash panel, engine to the passenger compartment | Harness Routing Views in Wiring Systems | --
S104 (V8 VIN G) | in the engine harness, approximately 14 cm (5.5 in) from the powertrain control module (PCM) breakout | -- | --
S104 (V6 VIN K) | In the engine harness, approximately 7 cm (2.3 in) from the right knock sensor breakout | -- | --
S107 (V8 VIN G) | In the engine harness, main branch, approximately 7 cm (2.8 in) from the powertrain control module (PCM) breakout | -- | --
S107 (V6 VIN K) | In the engine harness, main branch, approximately 21 cm (8.3 in) from the powertrain control module (PCM) breakout | -- | --
S110 (V8 VIN G) | In the engine harness, main branch, approximately 20 cm (7.9 in) from the powertrain control module (PCM) breakout | -- | --
S110 (V6 VIN K) | In the engine harness, approximately 4 cm (1.6 in) from the powertrain control module (PCM) breakout | -- | --
S121 (V6 VIN K) | In the engine harness, main branch, approximately 8 cm (3.1 in) from the powertrain control module (PCM) breakout | -- | --
S182 | In the forward lamp harness, approximately 15 cm (6 in) from the UH electrical center 1 breakout | -- | --
S207 | In the IP harness, main branch, approximately 4 cm (1.6 in) from the data link connector (DLC) breakout | -- | --
S215 | In the IP harness, main branch, approximately 11 cm (4 in) from the antenna cable breakout | -- | --
S234 (Automatic) | In the IP harness, main branch, approximately 5 cm (2 in) from the body control module (BCM) breakout | -- | --

## Automatic Transmission Components V8 VIN G

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Automatic Transmission (V6 VIN K) | Behind the engine | ABS Component Viewsin ABS Traction Control | --
Cruise Control/Clutch Anticipate Switch (V6 VIN K ) | Mounted in the clutch pedal bracket | Cruise Control Component Views in Cruise Control | Cruise Control Connector End Views in Cruise Control
Cruise Control (Clutch) Switch (V8 VIN G Manual) | Mounted in the clutch pedal bracket | Harness Routing Views in Wiring Systems | Cruise Control Connector End Views in Cruise Control
Park Neutral Position Switch | Under the center console, on the base of the shift control lever | -- | Engine Electrical Connector End Viewsin Starting and Charging
Powertrain Control Module (PCM) (V6 VIN K) | On the right side of the engine compartment, rear of the wheelhouse | Harness Routing Views in Wiring Systems |
Powertrain Control Module (PCM) (V8 VIN G) | On the right side of the engine compartment, rear of the wheelhouse | Engine Controls Component Views in Engine Controls 5.8L |
Second Gear Start Switch (V6 VIN K) (Chevrolet) | In the center of the IP, above the HVAC control | ABS Component Viewsin ABS Traction Control |
Stop Lamp Switch | Mounted on the brake pedal bracket | Cruise Control Component Views in Cruise Control |
Stop Lamp/TCC Switch (Automatic) | Mounted on the brake pedal bracket | -- | Lighting Systems Connector End Viewsin Lighting Systems
Underhood Electrical Center 2 | In the left front corner of the engine compartment | Engine Controls Component Views in Wiring Systems |
Vehicle Speed Sensor (Manual) | On the rear left side of the transmission | ABS Component Viewsin ABS Traction Control | Engine Controls Connector End Views in Engine Controls
Vehicle Speed Sensor (Automatic) | On the rear right side of the transmission | ABS Component Viewsin ABS Traction Control | Engine Controls Connector End Views in Engine Controls
C100 (10 cavities) | Engine to forward lamp harness, in the engine compartment, above the right wheelhouse | Harness Routing Views in Wiring Systems | Inline Harness Connector End Viewsin Wiring Systems
C105 (8 cavities) | Engine to forward lamp harness, in the engine compartment, above the right wheelhouse | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200A (17 cavities) | Forward lamp to IP harness, between the left kick panel and the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200B (18 cavities) | Forward lamp to IP harness, between the left kick panel and the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200D (48 cavities) | Part of the IP harness, between the left kick panel and the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C210 (10 cavities) | IP to engine harness, under the right side of the IP, behind the knee bolster | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C220 (10 cavities) | IP to engine harness, under the right side of the IP, behind the knee bolster | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C270 (2 cavities) | IP harness of the cruise control harness, near the brake/clutch pedal bracket | Harness Routing Views in Wiring Systems | --
G110 (V8 VIN G) | Attached to the rear of the left cylinder head | Harness Routing Views in Wiring Systems | --
G110 (V6 VIN K) | In the front of the engine, bolted to the pulley above the A/C clutch connector | Harness Routing Views in Wiring Systems | --
P100 | Left side in the dash panel, engine to the passenger compartment | Harness Routing Views in Wiring Systems | --
P110 | Right side in the dash panel, engine to the passenger compartment | Harness Routing Views in Wiring Systems | --
S104 (V8 VIN G) | in the engine harness, approximately 14 cm (5.5 in) from the powertrain control module (PCM) breakout | -- | --
S104 (V6 VIN K) | In the engine harness, approximately 7 cm (2.3 in) from the right knock sensor breakout | -- | --
S107 (V8 VIN G) | In the engine harness, main branch, approximately 7 cm (2.8 in) from the powertrain control module (PCM) breakout | -- | --
S107 (V6 VIN K) | In the engine harness, main branch, approximately 21 cm (8.3 in) from the powertrain control module (PCM) breakout | -- | --
S110 (V8 VIN G) | In the engine harness, main branch, approximately 20 cm (7.9 in) from the powertrain control module (PCM) breakout | -- | --
S110 (V6 VIN K) | In the engine harness, approximately 4 cm (1.6 in) from the powertrain control module (PCM) breakout | -- | --
S121 (V6 VIN K) | In the engine harness, main branch, approximately 8 cm (3.1 in) from the powertrain control module (PCM) breakout | -- | --
S182 | In the forward lamp harness, approximately 15 cm (6 in) from the UH electrical center 1 breakout | -- | --
S207 | In the IP harness, main branch, approximately 4 cm (1.6 in) from the data link connector (DLC) breakout | -- | --
S215 | In the IP harness, main branch, approximately 11 cm (4 in) from the antenna cable breakout | -- | --
S234 (Automatic) | In the IP harness, main branch, approximately 5 cm (2 in) from the body control module (BCM) breakout | -- | --