For 1990-2009 cars

# SERVICE GUILD: ENGINE OIL LEAK AT REAR MAIN SEAL

#### Subject: ENGINE OIL LEAK AT REAR MAIN SEAL (NEW PART)

#### Models Affected: 1987 - 1990 BONNEVILLE MODELS WITH 90 DEGREE V6 3.8, 3800 ENGINE

A new rear main oil rope seal has been released to service all 90 degree V6 3.8, 3800 type engines built through the 1990 model year. The part number for the seal is 24501340.

Parts are currently available from GMSPO.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.