For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Transaxle Oil SAE 75W85 Synthetic Lubricant Fluid GM P/N 12346190, or equivalent | 2.4 Liters | 2.5 Quarts

Application | Specification
--- | ---
Metric | English
Manual Transaxle Drain and Refill | 2.4 liters | 2.5 quarts
Recommended Transaxle Oil | GM Goodwrench Synthetic Manual Transmission Fluid, (GM P/N 12346190) or an equivalent SAE 75W-90 GL-4 Gear Oil.