For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Disc Brake Pad Lining Thickness (Minimum) | 1 mm | 0.04 in
Disc Brake Pad Lining and Plate Thickness (Minimum) | 6 mm | 0.24 in
Rotor Lateral Runout (Maximum) | 0.10 mm | 0.004 in
Rotor Surface Finish Scoring Depth (Maximum) | 0.38 mm | 0.015 in
Rotor Thickness (Minimum) | 15 mm | 0.59 in
Rotor Thickness Variation (Maximum) | 0.013 mm | 0.0005 in