For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Cooling System Capacity 1.0 L 3-Cylinder Engine

- Engine, Radiator and Heater Core

3.3 Liters

3.49 Quarts

- Coolant Recovery Reservoir

0.6 Liters

0.63 Quarts

- Total

3.9 Liters

4.13 Quarts

Cooling System Capacity 1.3 L 4-Cylinder Engine: Automatic Transaxle

- Engine, Radiator and Heater Core

4.13 Liters

4.37 Quarts

- Coolant Recovery Reservoir

0.6 Liters

0.63 Quarts

- Total

4.73 Liters

5.0 Quarts

Cooling System Capacity 1.3 L 4-Cylinder Engine: Manual Transmission:

- Engine, Radiator and Heater Core

4.0 Liters

4.23 Quarts

- Coolant Recovery Reservoir

0.6 Liters

0.63 Quarts

- Total

4.6 Liters

4.9 Quarts