For 1990-2009 cars

Fuse No. | Fuse Name | Fuse Description
--- | --- | ---
15A | A/C fuse | A/C 1 relay (compressor clutch), A/C 2 relay (condenser fan)
15A | ACC fuse | Cigar lighter, radio
15A | AIR BAG fuse | Inflatable restraint sensing and diagnostic module (SDM)
15A | BACK fuse | Backup lamp switch (manual transaxle), hazard switch, transaxle range switch (automatic transaxle)
20A | DEF fuse | Electronic brake control module (EBCM) (with ABS), electronic brake control relay (with ABS), lamp driver relay (with ABS), rear defogger switch
15A | DOME fuse | Data link connector - on board diagnostics II (DLC-OBD II), dome lamp, ignition key warning switch, luggage compartment lamp, powertrain control module (PCM), radio
20A | DOOR LOCK fuse | Power door lock control module
15A | F1 fuse | MAIN relay
15A | HAZARD fuse | Hazard switch, horn relay, electronic brake control module (EBCM) (with ABS)
15A | H/L, L fuse | High-beam indicator, LH headlamp, daytime running lamps (DRL) dode
15A | H/L, R fuse | RH headlamp, daytime running lamps (DRL) diode
20A | HEATER fuse | Blower speed selector switch, A/C 1 relay (compressor clutch)
15A | IG-COIL fuse | A/C amplifier, audio alarm module, camshaft position sensor, daytime running lamps (DRL) control module, engine cooling fan relay (RDTR), fuel pump relay, generator, heated oxygen sensor 1 and heated oxygen sensor 2 (H02S1 and H02S2), ignition Coil(s), IP indicators and gauges, noise suppressor filter, powertrain control module (PCM)
30A | PTC fuse | Early fuel evaporation (EFE) heater relay (PTC HTR)
30A | RDTR fuse | Engine cooling fan relay (RDTR)
15A | STOP fuse | Stoplamp switch
15A | TAIL fuse | Light 1 relay
15A | WIPER fuse | Front wiper motor, front wiper/washer switch, rear wiper motor, rear wiper/washer switch