For 1990-2009 cars

### Removal Procedure

1. Remove the following components from the rear bumper fascia:

1.1. | The 2 screws

1.2. | The rear license plate lamp (3)

2. Remove the bulb socket (1) from the rear license plate lamp (3).
3. Remove the bulb (2) from the socket (1) of the rear license plate lamp.

### Installation Procedure

1. Install the bulb (2) to the socket (1) of the rear license plate lamp.
2. Install the socket (1) to the rear license plate lamp (3).
3. Install the lamp (3) to the rear bumper fascia. Secure the lamp with the 2 screws.