For 1990-2009 cars

Condition | Possible Cause
--- | ---
Harsh engagement into any forward range |

• | Low fluid

• | TV cable out of adjustment, binding or damaged

• | Shift select cable out of adjustment, biding or damaged

• | Manual valve binding or sticking

• | Throttle valve binding or sticking

• | B2 control valve binding or sticking

• | Accumulator(s) pistons damaged or leaking

• | Accumulator(s) seals cut or damaged

• | Accumulator(s) broken or distorted springs

• | Incorrect line pressure