For 1990-2009 cars

Figure 1: |

#### Cowl

(1) | Supplemental Inflatable Restraint (SIR) Harness
(2) | Duty Check Data Link Connector
(3) | Inflatable Restraint IP Module Connector
(4) | Engine Wiring Harness
(5) | Powertrain Control Module (PCM) C1
(6) | Powertrain Control Module (PCM) C2
(7) | Powertrain Control Module (PCM) C3
(8) | Junction Block
(9) | Turn Signal/ Combination Switch Connector
(10) | Floor Harness
(11) | Power Door Lock Control Module
(12) | Main Wiring Harness
(13) | Electronic Brake Control Module (EBCM) C1 with ABS
(14) | Electronic Brake Control Module (EBCM) with ABS
(15) | Electronic Brake Control Module (EBCM) C2 with ABS
(16) | Lamp Driver Relay (with ABS)
(17) | Clutch Pedal Position (CPP) Switch (Manual Transaxle)
(18) | Stoplamp Switch
(19) | Daytime Running Lamps (DRL) Control Module

Figure 2: |

#### LH/RH Front Door Wiring (4-Door)

(1) | LH/RH Power Door Lock Switch Connector (4-Door With Power Door Locks)
(2) | LH/RH Front Power Door Lock Actuator Connector (4-Door With Power Door Locks)
(3) | LH/RH Front Speaker

Figure 3: |

#### LH/RH Rear Door (4-Door)

(1) | LH/RH Rear Power Door Lock Actuator (With Power Door Locks)