For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Data Link Connector (DLC) OBD 2 | Below the left side of the IP, near the center console | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
Inflatable Restraint Forward Discriminating Sensor | The front center of the grille, behind the hood latch assembly | SIR Component Views | --
Inflatable Restraint IP Module | The top of the right side of the IP, above the glove box | SIR Component Views | SIR Connector End Views
Inflatable Restraint Sensing and Diagnostic Module (SDM) | The center of the console, in front of the manual selector | SIR Component Views | SIR Connector End Views
Inflatable Restraint Steering Wheel Module | The center of the steering wheel behind the steering-wheel center pad | -- | --
Instrument Panel Cluster Assembly | The left side of the IP | -- | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Junction Block | Behind the left side of the IP | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Seat Belt Switch | In the left seat belt buckle | -- | Audible Warnings Connector End Views Instrument Panel, Gauges and Console
Supplemental Inflator Restraint Data Link Connector (SIR DLC) | Behind the left lP near the junction block | -- | Data Link Communications Connector End Views in Data Link Communications
Turn Signal/Combination Switch | On the steering column | -- | Lighting Systems Connector End Views in Lighting Systems
C203 (13 Cavities) | The I/P harness to the floor harness, behind the left side of the IP, near the junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C210 (5 Cavities) | The supplemental inflatable restraint (SIR) harness to the IP harness, behind the left side of the IP, near the junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G204 | Behind the right side of the kick panel | -- | --
G400 | The rear center of the luggage compartment (2-Door) | Harness Routing Views in Wiring Systems | --
The rear center of the luggage compartment (4-Door) | Harness Routing Views in Wiring Systems | --
P203 | Behind the right kick panel | -- | --
S227 | The IP harness, approximately 5 cm (2 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S241 | The IP harness, approximately 5 cm (2 in) from the breakout of the IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S242 | The IP harness, at the breakout of the IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S249 | The IP harness, approximately 1 cm (0.375 in) from the breakout of the IP cluster assembly connector C2 | Harness Routing Views in Wiring Systems | --