For 1990-2009 cars

Application | Fluid/Lubricant
--- | ---
Engine Oil | The engine oil with the American Petroleum Institute Certified For Gasoline Engines Starburst symbol of the proper viscosity. To determine the preferred viscosity for your vehicle's engine, see Explanation of Scheduled Services
Engine Coolant | A 50/50 mixture of clean water (preferably distilled) and good quality Ethylene Glycol Base Coolant (GM Part No. 1052753 or equivalent) conforming to GM Specification 1825M or approved recycled coolant conforming to GM Specification 1825M. See Explanation of Scheduled Services
Hydraulic Brake System | Delco Supreme 11® Brake Fluid (GM P/N 12377967) or equivalent DOT-3 brake fluid
Parking Brake Cable Guides | Chassis Lubricant (GM P/N 12377985) or lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB
Power Steering System | GM Power Steering Fluid (GM Part No. 1052884 - 1 pint, 1050017 - 1 quart, or equivalent).
Manual Transaxle | GM Goodwrench Synthetic Manual Transmision Fluid (GM Part No. 12346190 - 1 quart) or equivalent SAE 75W-910 GL-4 Gear Oil.
Automatic Transaxle | DEXRON®-III Automatic Transmission Fluid.
Key Lock Cylinders | Multi-Purpose Lubricant, Superlube® (GM P/N 12346241 or equivalent)
Manual Transaxle Shift Linkage | Chassis Lubricant (GM P/N 12377985 or equivalent) or lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB
Clutch Linkage Pivot Points | Chassis Lubricant (GM P/N 12377985) or lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB
Chassis Lubrication | Chassis Lubricant (GM P/N 12377985) or lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB
Windshield Washer Solvent | GM Optikleen ® Washer Solvent (GM Part No.1051515) or equivalent.
Hood and Door Hinges | Multi-Purpose Lubricant, Superlube® (GM Part No. 12346241 or equivalent).
Weatherstrip Conditioning | Dielectric Silicone Grease (GM Part No. 12345579 or equivalent).