For 1990-2009 cars

### Removal Procedure

The diode module is located under the glove box and next to the cigarette lighter.

1. Cut the electrical tape that is securing the diode module (1) to the main wire harness.
2. Open the cover at the end of the diode module electrical connector.
3. Remove the diode module circuit board (1) from the diode module electrical connector (2).

### Installation Procedure

1. Insert the diode module circuit board (1) into the diode module electrical connector (2).
2. Close the cover of the diode module electrical connector.
3. Secure the diode module (1) to the main wire harness with an electrical tape.