For 1990-2009 cars

DTC | Description | Type | Illuminate MIL
--- | --- | --- | ---
P0106 | Manifold Absolute Pressure (MAP) Sensor System Performance | B | Yes
P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | A | Yes
P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | A | Yes
P0111 | Intake Air Temperature (IAT) Sensor Performance | B | Yes
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | A | Yes
P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | A | Yes
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | A | Yes
P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | A | Yes
P0121 | Throttle Position (TP) Sensor System Performance | B | Yes
P0122 | Throttle Position (TP) Sensor Circuit Low Voltage | A | Yes
P0123 | Throttle Position (TP) Sensor Circuit High Voltage | A | Yes
P0125 | Engine Coolant Temperature (ECT) Excessive Time To Closed Loop Fuel Control | B | Yes
P0131 | Heated Oxygen Sensor (HO2S) Circuit Low Voltage -- Sensor 1 | B | Yes
P0132 | Heated Oxygen Sensor (HO2S) Circuit High Voltage -- Sensor 1 | B | Yes
P0133 | Heated Oxygen Sensor (HO2S) Slow Response -- Sensor 1 | B | Yes
P0134 | Heated Oxygen Sensor (HO2S) Circuit Insufficient Activity -- Sensor 1 | B | Yes
P0135 | Heated Oxygen Sensor (HO2S) Heater Circuit -- Sensor 1 | B | Yes
P0136 | Heated Oxygen Sensor (HO2S) Circuit -- Sensor 2 | B | Yes
P0141 | Heated Oxygen Sensor (HO2S) Heater circuit -- Sensor 2 | B | Yes
P0171 | Fuel Trim System Lean | B | Yes
P0172 | Fuel Trim System Rich | B | Yes
P0300 | Engine Misfire Detected | B | Yes
P0301 | Cylinder 1 Misfire Detected | B | Yes
P0302 | Cylinder 2 Misfire Detected | B | Yes
P0303 | Cylinder 3 Misfire Detected | B | Yes
P0335 | Crankshaft Position (CKP) Sensor Circuit | A | Yes
P0340 | Camshaft Position (CMP) Sensor Circuit | A | Yes
P0400 | Exhaust Gas Recirculation (EGR) System | B | Yes
P0420 | Three Way Catalyst (TWC) System Low Efficiency | B | Yes
P0443 | Evaporative Emission (EVAP) System Incorrect Purge Flow | B | Yes
P0461 | Fuel Level Sensor Circuit Performance | B | Yes
P0463 | Fuel Level Sensor Circuit High Voltage | B | Yes
P0480 | Cooling Fan Control Circuit | B | Yes
P0500 | Vehicle Speed Sensor (VSS) Circuit | B | Yes
P0505 | Idle Control System | A | Yes
P0506 | Idle Speed Low | B | Yes
P0507 | Idle Speed High | B | Yes
P0510 | Closed Throttle Position (CTP) Switch Circuit | B | Yes
P0601 | Powertrain Control Module (PCM) Memory | B | Yes
P0603 | Powertrain Control Module (PCM) Memory Reset | B | Yes
P1250 | Early Fuel Evaporation (EFE) Heater Circuit | B | Yes
P1450 | Barometric Pressure Sensor Circuit | A | Yes
P1451 | Barometric Pressure Sensor Performance | B | Yes
P1500 | Starter Signal Circuit | B | Yes
P1510 | Back Up Power Supply | A | Yes
P1530 | Ignition Timing Adjustment Switch Circuit | A | Yes