For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Junction Block | Behind left side of the IP | Power and Grounding Component Views | Power and Grounding Connector End Views
LH Front Power Door Lock Actuator (4-Door With Power Door Locks) | Left front door on door latch assembly | Power Door Systems Component Views | Power Door Systems Connector End Views
LH Power Door Lock Switch (4-Door With Power Door Locks) | Left front door trim panel | Power Door Systems Component Views | Power Door Systems Connector End Views
LH Rear Power Door Lock Actuator (4-Door with Power Door Locks) | Left rear door, on door latch assembly | Power Door Systems Component Views | Power Door Systems Connector End Views
Power Door Lock Control Module (4-Door with Power Door Locks) | Left side of the IP, mounted to A-pillar, above the left kick panel | Power Door Systems Component Views | Power Door Systems Connector End Views
RH Front Power Door Lock Actuator (4-Door with Power Door Locks) | Right front door, on the door latch assembly | Power Door Systems Component Views | Power Door Systems Connector End Views
RH Power Door Lock Switch (4-Door With Power Door Locks) | In the right front door trim panel | Power Door Systems Component Views | Power Door Systems Connector End Views
RH Rear Power Door Lock Actuator (4-Door with Power Door Locks) | Right rear door, on the door latch assembly | Power Door Systems Component Views | --
C212 (6 Cavities) (4-Door) | Floor harness to left front door, behind the left kick panel | Harness Routing Views | Inline Harness Connector End Views
C213 (6 Cavities) (4-Door) | Floor harness to right front door, behind right kick panel | Harness Routing Views | Inline Harness Connector End Views
C306 (2 Cavities) (4-Door With Power Door Locks) | Floor harness to the left rear door harness, attached to left side B-pillar | Harness Routing Views | Inline Harness Connector End Views
C307 (2 Cavities) (4-Door With Power Door Locks) | Floor harness to the right rear door harness, attached to right side B-pillar | Harness Routing Views | Inline Harness Connector End Views
G203 | Junction block case ground, under the left side of the IP | -- | --
P304 (4-Door With Power Door Locks) | Right rear door jamb | -- | --
P500 | Left front door | -- | --
P600 | Right front door | -- | --
P700 (4-Door With Power Door Locks) | Left rear Door | -- | --
P800 (4-Door With Power Door Locks) | Right rear door | -- | --
S307 (4-Door With Power Door Locks) | Floor harness, approximately 5 cm (2 in) from the power door lock control module connector breakout | Harness Routing Views | --
S308 (4-Door With Power Door Locks) | Floor harness, approximately 10 cm (4 in) from the power door lock control module connector breakout | Harness Routing Views | --
S314 (4-Door With Power Door Locks) | Floor harness, approximately 25 cm (10 in) from the C201 breakout | Harness Routing Views | --