For 1990-2009 cars

The receiver-dryer mounts to the front of the condenser. The receiver-dryer is connected to the condenser outlet pipe (1) between the condenser and the evaporator.

The receiver-dryer performs the following functions:

• | The receiver-dryer serves as a temporary storage container for condensed liquid refrigerant.

• | The receiver-dryer acts as a filter which removes moisture and contaminants from the system.