For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Brake Fluid Level Switch | In the brake fluid reservoir | -- | Hydraulic Brake Connector End Views
Daytime Running Lamps (DRL) Control Module | Behind the left side of the IP | Lighting Systems Component Views | Lighting Systems Connector End Views
Ignition Switch | Right side of the steering column | -- | --
Instrument Panel Cluster Assembly | Left side of the IP | -- | Instrument Panel, Gages, and Console Connector End Views
Junction Block | Behind left side of the IP | Power and Grounding Component Views | Power and Grounding Connector End Views
Parking Brake Switch | Passenger compartment, behind manual selector | Instrument Panel, Gages, and Console Component Views | --
C200 (12 Cavities) | Main harness to the IP harness, behind the left IP, near junction block | Harness Routing Views | Inline Harness Connector End Views
C201 (14 Cavities) | Main harness to the floor harness, behind the left side of the IP, near junction block | Harness Routing Views | Inline Harness Connector End Views
G102 | Left front side of the engine compartment on the left front inner fender near battery | Harness Routing Views | --
G203 | Junction block case ground, under the left side of the IP | -- | --
P200 | Left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views | --
S207 | Main harness, approximately 12 cm (5 in) from the G201 breakout | -- | --
S213 | Main harness, approximately 8 cm (3.125 in) from P200 | -- | --
S223 | Main harness, approximately 10 cm (4 in) from P200 | -- | --
S241 | IP harness, approximately 5 cm (2 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views | --
S242 | IP harness, at the IP cluster assembly connector C3 breakout | Harness Routing Views | --
S247 | Main harness, approximately 18 cm (7.06 in) from P200 | -- | --