For 1990-2009 cars

Cause | Action
--- | ---
The shear bolts are damaged. | Replace the shear bolts.
The housing assembly is damaged. | Replace the steering column.
The shift linkage is not adjusted properly. | Adjust the shift linkage adjustment.
The brake transmission shift interlock (BTSI) system is damaged. | Repair or replace the BTSI as needed.
The shaft assembly is damaged. | Replace the steering column as needed.
The ignition switch assembly is damaged. | Replace the ignition switch assembly.
The key is incorrect, bent, or twisted. | Replace the key.
The park lock cable is not adjusted properly. | Adjust the park lock cable.
The shift lever is not in the P position. | Place the gear shift in the P position.