For 1990-2009 cars

### Removal Procedure

1. Open the instrument panel compartment (3).
2. Remove the instrument panel compartment lock (2) from the instrument panel compartment (3) by removing the 2 screws (1).

### Installation Procedure

1. Install the instrument panel compartment lock (2) to the instrument panel compartment (3). Secure the lock with the 2 screws (1).
2. Close the instrument panel compartment (3).