For 1990-2009 cars

### Removal Procedure

1. Disconnect the accelerator control cable (1) from the accelerator pedal assembly (2).
2. Remove the C-clip (3) from the accelerator pedal assembly pivot.
3. Remove the accelerator pedal assembly (2) and spring from the mounting bracket (4).

### Installation Procedure

1. Install the accelerator pedal assembly (2) and spring to the mounting bracket (4).
2. Install the C-clip (3) to the accelerator pedal assembly pivot.
3. Connect the accelerator control cable (1) to accelerator pedal assembly (2).