For 1990-2009 cars

The horn is located under the hood. The horn is attached to the left side of the radiator core support. The horn actuates by depressing the horn buttons.

The horn buttons are located on the edge of the steering wheel. The horn buttons are incorporated into the steering wheel pad. The horn buttons are not serviceable. If the horn buttons are defective, replace the steering wheel pad.