For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Audio Alarm Module | Left side of the lower IP, left of Steering column | Audible Warnings Component Views | Audible Warnings Connector End Views
Instrument Panel Cluster Assembly | Left side of the IP | -- | Instrument Panel, Gages, and Console Connector End Views
Junction Block | Behind left side of the IP | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
LH Front Door Jamb Switch | Left front door frame, in lower rear corner | Lighting Systems Component Views in Lighting Systems | --
Seat Belt Switch | In left seat belt buckle | -- | Audible Warnings Connector End Views
C203 (13 Cavities) | I/P harness to floor harness, behind left side of the IP, near junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G400 (2-Door) | Rear center of luggage compartment | Harness Routing Views in Wiring Systems | --
(4-Door) | Rear center of luggage compartment | Harness Routing Views in Wiring Systems | --
S217 | IP harness, at the C200 breakout | Harness Routing Views in Wiring Systems | --
S227 | IP harness, approximately 5 cm (2 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S235 | IP harness, approximately 5 cm (2 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S241 | IP harness, approximately 5 cm (2 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views in Wiring Systems | --
S242 | IP harness, at the IP cluster assembly connector C3 breakout | Harness Routing Views in Wiring Systems | --