For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Refrigerant-134a System Capacity | 500-600 g | 1.10-1.32 lbs
Refrigerant Oil Capacity - Polyalkylene Glycol (PAG) | 100 ml | 3.4 fl oz
Refrigerant Oil Capacity - Polyalkylene Glycol (PAG) If Replacing the Condenser | 20-30 ml | 0.7-1 fl oz
Refrigerant Oil Capacity - Polyalkylene Glycol (PAG) If Replacing the Receiver-Dryer | 10 ml | 0.3 fl oz