For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ball Joint Nut and Bolt | 60 N·m | 44 lb ft
Control Arm Front Bracket Bolt | 90 N·m | 66 lb ft
Control Arm Rear Bracket Bolt | 43 N·m | 32 lb ft
Drive Axle Nut | 175 N·m | 129 lb ft
Front Control Arm Bracket Nut | 125 N·m | 92 lb ft
Stabilizer Shaft Link Nut | 28 N·m | 20 lb ft
Stabilizer Shaft Link-to-Stabilizer Shaft Nut | 50 N·m | 38 lb ft
Stabilizer Shaft Mounting Brackets Bolt | 28 N·m | 20 lb ft
Strut Nut | 50 N·m | 37 lb ft
Strut-to-Knuckle Bolts and Nut | 80 N·m | 59 lb ft
Tie Rod End Castle Nut | 43 N·m | 32 lb ft
Upper Strut Support Nut | 28 N·m | 21 lb ft
Wheel Speed Sensor Harness Bolt | 10 N·m | 89 lb in
Wheel Speed Sensor Retaining Bolt | 10 N·m | 89 lb in