For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Door-to-Hinge Bolts | 34 N·m | 25 lb ft
Front Door Window Screws | 5 N·m | 44 lb in
Hinge-to-Door Jamb Bolts | 34 N·m | 25 lb ft
Outside Handle-to-Door Nuts | 7 N·m | 62 lb in
Rear Door Window Screws | 5 N·m | 44 lb in
Regulator-to-Window Mounting Nuts | 5 N·m | 44 lb in
Window Hardware Mounting Screws and Bolts | 5 N·m | 44 lb in