For 1990-2009 cars

The component location table shows a list of all the electrical components within a systems electrical schematics. The table consists of the following information within a system's electrical schematic:

• | All components

• | Grounds

• | Pass-through grommets

• | Splices

The table consists of 4 columns which describe the following information:

• | The component name

• | The component location

• | The reference to the component view

• | The reference to the connector end view (if applicable)

### Name

The name cells provide the name of the components that are used on the schematic(s). If a connector is listed the number of cavities are also provided. This represents the total number of cavities in the connector regardless of how many connectors are actually used.

### Location

The location cell provides a written location of where the component is in the vehicle with respect to vehicle landmarks. Nearly all of the following information shown on a schematic can be pinpointed visually using the component location view illustrations:

• | Components

• | Connectors

• | Grounds

• | Splices

### Locator View

This column contains the reference to the appropriate component view. The reference contains the location within the subsection and the section. Refer to How to Use Component Location Views .

### Connector End View

This column contains the reference to the appropriate connector end view. The reference contains the location within the subsection and the section. Refer to How to Use Connector End Views .