For 1990-2009 cars

The belt-driven water pump (2) is a centrifugal type pump.

The belt-driven water pump consists of the following components:

• | An impeller

• | A drive shaft

• | A drive belt pulley

The water pump is mounted on the front of the transverse-mounted engine, and shares its drive belt with the generator. The impeller is supported by a completely sealed bearing. The water pump is serviced as an assembly and, therefore, cannot be disassembled.