For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Direct Clutch Solenoid | Left rear side of the transaxle, attached to the valve body | -- | --
Junction Block | Behind left side of the IP | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Powertrain Control Module (PCM) | Behind the right side of the IP, near the glove box | Engine Controls Component Views in Engine Controls | Powertrain Control Module Connector End Views in Engine Controls
2nd Brake Solenoid | Left rear side of transaxle attached to valve body | -- | --
Transaxle Range Switch | Left side of the engine compartment, mounted to top of the transaxle | -- | Automatic Transmission Connector End Views
Vehicle Speed Sensor (VSS) | Left side of the engine compartment, top of the transaxle | -- | --
C108 (2 Cavities) | Engine harness to the transaxle solenoid jumper, left rear side of transaxle | Harness Routing Views in Wiring Systems | --
C112 (16 Cavities) | Main harness to engine harness, right rear side of the engine compartment near bulkhead | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G104 | Center rear side of the engine on the intake manifold | Harness Routing Views in Wiring Systems | --
P200 | Left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views in Wiring Systems | --
P202 | Center of the engine compartment, on the bulkhead | Harness Routing Views in Wiring Systems | --
S101 | Main harness, approximately 11 cm (4.5 in) from the brake fluid level switch breakout | Harness Routing Views in Wiring Systems | --
S126 | Engine harness, approximately 8 cm (3.1 in) from P202 | Harness Routing Views in Wiring Systems | --
S130 | Engine harness, approximately 5 cm (2 in) from starter breakout | Harness Routing Views in Wiring Systems | --
S152 | Main harness, approximately 19 cm (7.4 in) from the C113 breakout | Harness Routing Views in Wiring Systems | --
S154 | Engine Harness, approximately 9 cm (3.6 in) from P202 | Harness Routing Views in Wiring Systems | --
S158 | Engine harness, approximately 19 cm (1.5 in) from P202 | -- | --
S165 | Engine harness, approximately 5 cm (2 in) from the starter breakout | Harness Routing Views in Wiring Systems | --
S202 | Main harness, approximately 8 cm (3.125 in) from the junction block connector C6 breakout | -- | --
S231 | Main harness, approximately 15 (6 in) cm from P200 | -- | --
S248 | Engine harness, approximately 4 cm (2 in) from the powertrain control module (PCM) connector C1 breakout | Harness Routing Views in Wiring Systems | --
S263 | Engine harness, approximately 3 cm (1.9 in) from the C205 breakout | Harness Routing Views in Wiring Systems | --