For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Cleaner Stud Bracket Bolts | 10 N·m | 89 lb in
Crankshaft Position (CKP) Sensor Bolt | 10 N·m | 89 lb in
Distributor Flange Bolts | 15 N·m | 11 lb ft
ECT Sensor | 12.5-17.5 N·m | 9.5-12.5 lb ft
EGR Valve Bolts | 20 N·m | 15 lb ft
EVAP Canister Purge Valve Bracket Bolts | 11 N·m | 8 lb ft
EVAP Tank Pressure Control Solenoid Valve Bolt | 1.6 N·m | 14 lb in
Fuel Limiter Vent Valve (FLVV) Bolts | 1.6 N·m | 12 lb in
Fuel Pipe Guard Nuts | 15 N·m | 11 lb ft
Fuel Sender Assembly Bolts | 10 N·m | 89 lb in
Fuel Pipe Guard Nuts | 15 N·m | 11 lb ft
Fuel Tank Mounting Bolts | 25 N·m | 18 lb ft
Fuel Tank Pressure Control Valve Attaching Screw | 1.2-2.0 N·m | 11-18 lb in
Fuel Tank Pressure Sensor Bolts | 1.2-2.0 N·m | 11-18 lb in
Fuel Vapor Separator Bolts | 1.2-2.0 N·m | 11-18 lb in
HO2S 1 | 40-50 N·m | 29-36 lb ft
HO2S 2 | 40-50 N·m | 29-36 lb ft
ISC Motor Screws | 2.8-4.0 N·m | 24-36 lb in
MAP Sensor Bracket Bolts | 10 N·m | 89 lb in
Negative Battery Cable-to-Negative Battery Terminal Retainer | 5.5 N·m | 49 lb in
Parking Brake Cable Bracket Bolt | 15 N·m | 11 lb ft
PCM Bracket Bolts | 6 N·m | 54 lb in
Spark Plugs | 28 N·m | 20 lb ft
Throttle Body Fuel Injection (TBI) Unit Bolts | 23 N·m | 17 lb ft
TBI Unit Upper Assembly to Lower Assembly Bolts | 3.5 N·m | 31 lb in
TP Sensor Bolts | 2.0 N·m | 18 lb in
Vehicle Speed Sensor (A/T) Bolt | 8 N·m | 72 lb in