For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel cluster. Refer to Instrument Cluster Replacement .
2. Remove the bulb sockets (3,4) from the back of the cluster (6), as needed.
3. Remove the bulbs (2,5) from the bulb sockets (3,4), as needed.

### Installation Procedure

1. Install any bulbs (2,5) to the bulb sockets (3,4) that were removed.
2. Install the bulb sockets (3,4) to the back of the cluster (6) that were removed.
3. Install the instrument panel cluster. Refer to Instrument Cluster Replacement .