For 1990-2009 cars

The optional rear window defogger system consists of the following components:

• | A rear window defogger switch

• | A rear window that has the following lines on the inside surface of the rear window:

- | Several horizontal ceramic silver compound element lines (4)

- | 2 vertical bus bars (6)

• | The feed terminal (+) (5) is soldered to the bus bar on the right side.

• | The ground terminal (-) (7) is soldered to the bus bar on the left side.