For 1990-2009 cars

Inspect the following components:

• | The wheel alignment

• | The wheel bearings for wear or damage

• | The joints from the column to the steering gear for free movement

• | The joints from the column to the steering gear for secure installation

• | The tie rod ends for free movement

• | The ball joints for free movement

• | The steering shaft bearings for free movement

• | The steering gear for the proper operation