For 1990-2009 cars

Figure 1: |

#### Component Location - Information Sensors/Input Devices

(1) | MAP Sensor
(2) | HO2S 2
(3) | VSS M/T (part of speedometer)
(4) | VSS A/T
(5) | Transmission range switch (A/T only)
(6) | ECT Sensor
(7) | CMP Sensor
(8) | HO2S 1
(9) | CKP Sensor
(10) | PSP Switch
(11) | IAT Sensor
(12) | TP Sensor
(13) | A/C Compressor Control Module
(14) | Diode Module (electrical load signal)
(15) | Fuel Tank Pressure Sensor
(16) | Fuel Level Sensor

Figure 2: |

#### Component Location - PCM Controlled Devices

(1) | EVAP Canister Purge Valve
(2) | Malfunction Indicator Lamp (MIL)
(3) | Upshift Indicator Lamp (M/T only)
(4) | Cooling Fan Control Relay
(5) | Fuel Pump Relay
(6) | Ignition Coil #1
(7) | Fuel Injectors
(8) | Ignition Coil #2
(9) | EVAP Canister Vent Valve
(10) | EVAP Tank Pressure Control Solenoid Valve
(11) | IAC Valve

Figure 3: |

#### Component Location - Other Components

(1) | Data Link Connector (DLC)
(2) | Junction Block (fuse block)
(3) | Main Relay
(4) | Battery
(5) | Duty Check Data Link Connector
(6) | PCM
(7) | EVAP Canister

Figure 4: |

#### Ignition Coils, CMP Sensor and PCV Valve

(1) | CMP Sensor
(2) | Ignition Coil #1 (Cylinders 1 and 4)
(3) | Ignition Coil #2 (Cylinders 2 and 3)
(4) | PCV Valve