For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the system check? | -- | Go to Step 2 | Go to Radio/Audio System Check
2 | Inspect the cassette player door for an obstruction. Is an obstruction present? | -- | Go to Step 3 | Go to Step 4
3 | Remove the obstruction. Is the repair complete? | -- | Go to Step 5 | --
4 | Replace the radio. Refer to Radio Replacement . Is the repair complete? | -- | Go to Radio/Audio System Check | --
5 |

1. Inspect and clean the tape head
2. Insert the diagnostic test tape.

Does the cassette player operate correctly?

--

Go to Radio/Audio System Check

Go to Step 6

6 | Replace the radio. Refer to Radio Replacement . Is the repair complete? | -- | Go to Radio/Audio System Check | --