For 1990-2009 cars

Causes | Correction
--- | ---
Sticky caliper or caliper pistons | Repair or replace the caliper.
Contaminated or improper brake fluid | Flush the brake system and repair the affected brake components.
Uneven brake lining material | Replace the brake linings.
Loose front or rear brake assembly attachment | Locate and tighten the loose brake components.
Restricted brake fluid passage | Locate and repair the source of the brake fluid restriction.
Improperly adjusted stoplamp switch | Adjust the stoplamp switch to specification.
Brake pedal linkage interference/binding | Repair or replace the brake pedal linkage.
Improperly adjusted parking brake | Adjust the parking brake.
Loose front suspension parts | Locate and tighten, repair or replace the loose front suspension components.
Operator riding brake pedal | Advise the operator of the proper brake usage.