For 1990-2009 cars

Table 1: | Cigar Lighter
Table 2: | Fuse Box C1
Table 3: | Fuse Box C4
Table 4: | Junction Block C1
Table 5: | Junction Block C2
Table 6: | Junction Block C3
Table 7: | Junction Block C4
Table 8: | Junction Block - C5
Table 9: | Junction Block - C6
Table 10: | Junction Block - C7
Table 11: | Junction Block C8

#### Cigar Lighter

Connector Part Information |

• | 09705 021A0 15

• | GRY

Pin | Wire Color | Function
--- | --- | ---
A | WHT/BLK | Ignition Positive Voltage
B | BLK | Ground

#### Fuse Box C1

Connector Part Information |

• | 09705 03025 20

• | WHT

Pin | Wire Color | Function
--- | --- | ---
1 | BLK/BLU | Battery Positive Voltage
2 | WHT/RED | Battery Positive Voltage
3 | WHT | Battery Positive Voltage

#### Fuse Box C4

Connector Part Information |

• | 09705 02905 21

• | BLK

Pin | Wire Color | Function
--- | --- | ---
1 | WHT/GRN | Battery Positive Voltage
2 | WHT/YEL | Battery Positive Voltage

#### Junction Block C1

Connector Part Information |

• | 09703 00000 00

• | BLK

Pin | Wire Color | Function
--- | --- | ---
1 | RED/YEL | Ignition Positive Voltage
2 | RED/GRN | Ignition Positive Voltage
3 | WHT | Battery Positive Voltage

#### Junction Block C2

Connector Part Information |

• | 09704 00000 00

• | BLK

Pin | Wire Color | Function
--- | --- | ---
1 | -- | Not Used
2 | BLU | Ignition Positive Voltage
3 | BLK | Ground
4 | -- | Not Used
5 | GRN | Battery Positive Voltage
6 | BLK/WHT | Ignition Positive Voltage
7 | GRN | Key-In Signal
8 | BLK | BRAKE Indicator Control

#### Junction Block C3

Connector Part Information |

• | NFV12FB

• | WHT

Pin | Wire Color | Function
--- | --- | ---
1 | GRN/YEL | Turn Signal Switch On RH
2 | GRN/RED | Turn Signal Switch On LH
3 | GRN | Turn Relay/Turn Signal Switch
4 | YEL/BLU | Turn Relay/Hazard Switch Off
5 | BLU/BLK | Horn Relay/SIR Contact Coil
6 | RED | Dimmer Switch - Pass
7 | YEL/BLU | Front Wiper Switch/Wiper Fuse
8 | YEL | BACK Fuse
9 | BLK | Ground
10 | WHT | Light Switch Off
11 | RED/BLK | Dimmer Switch Ground
12 | WHT/GRN | Hazard Fuse

#### Junction Block C4

Connector Part Information |

• | 0970520WB120

• | BLK

Pin | Wire Color | Function
--- | --- | ---
1 | YEL/BLK | Air Bag Fuse
2 | -- | Not Used
3 | BLK/WHT | IG - Coil Fuse
4 | YEL/BLU | Wiper Fuse
5 | -- | Not Used
6 | GRN/RED | LH Turn Signal
7-8 | -- | Not Used
9 | GRN/YEL | RH Turn Signal
10 | RED/YEL | Light 1 Relay Output
11 | -- | Not Used
12 | WHT/BLK | ACC Fuse
13 | BRN/BLK | Ignition Switch Bulb Test
14 | BLU/BLK | DOME Fuse
15 | LT GRN | Heater Fuse
16 | BLK | Ground - G203
17 | YEL/GRN | DEF Fuse
18 | WHT | DOME Fuse
19 | WHT/BLU | H/L, L Fuse
20 | RED | Dimmer Switch/High Beam Indicator

#### Junction Block - C5

Connector Part Information |

• | 0970506VB020

• | BLK

Pin | Wire Color | Function
--- | --- | ---
1 | WHT/GRN | HAZARD Fuse
2 | RED/YEL | Light 1 Relay
3 | GRN | Horn Relay
4 | GRN/RED | LH Front Park/Turn Lamp
5 | GRN/YEL | RH Front Park/Turn Lamp
6 | RED | Headlamps

#### Junction Block - C6

Connector Part Information |

• | 0970518WB120

• | BLK

Pin | Wire Color | Function
--- | --- | ---
1-4 | -- | Not Used
5 | WHT | DOME Fuse
6 | -- | Not Used
7 | YEL | Back Fuse
8 | YEL/BLU | Wiper Fuse
9 | BLK/WHT | IG - Coil Fuse
10 | WHT/YEL | STOP Fuse
11 | WHT | Tail Fuse
12 | WHT/RED | H/L, R Fuse
13 | WHT/BLU | H/L, L Fuse
14 | BLK | Ground - G203
15 | BLK/RED | Ignition Switch Start Signal
16 | -- | Not Used
17 | YEL/GRN | Def. Fuse
18 | LT GRN | Heater Fuse

#### Junction Block - C7

Connector Part Information |

• | 0970502MB020

• | BLK

Pin | Wire Color | Function
--- | --- | ---
1 | WHT/GRN | Ignition Fuse
2 | WHT/YEL | Lamp Fuse

#### Junction Block C8

Connector Part Information |

• | 09705 12VB2 20

• | BLK

Pin | Wire Color | Function
--- | --- | ---
1 | GRN/YEL | Right Turn Signal
2 | RED/YEL | Light 1 Relay Output
3 | BLK | Not Used
4 | YEL/BLU | Ignition Positive Voltage
5 | -- | Not Used
6 | WHT | Battery Positive Voltage on a 4-Door
7 - 9 | -- | Not Used
10 | RED | Left Turn Signal
11 - 12 | -- | Not Used