For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Automatic Transaxle

- Drain and Refill

1.5 liters

1.6 quarts

- Overhaul w/o Torque Converter

3.5 liters

3.7 quarts

- Overhaul w/ Torque Converter

4.9 liters

5.2 quarts

Manual Transaxle

- Drain and Refill

2.4 liters

2.5 quarts

Cooling System Capacity 1.0L (3-Cyl Engine)

- Engine, Radiator and Heater Core

3.3 liters

3.49 quarts

- Coolant Recovery Reservoir

0.6 liters

0.63 quarts

- Total

3.9 liters

4.13 quarts

Cooling System Capacity 1.3L (4-Cyl w/ Automatic Transaxle)

- Engine, Radiator and Heater Core

4.13 liters

4.37 quarts

- Coolant Recovery Reservoir

0.6 liters

0.63 quarts

- Total

4.73 liters

5.0 quarts

Cooling System Capacity 1.3L (4-Cyl w/ Manual Transaxle)

- Engine, Radiator and Heater Core

4.0 liters

4.23 quarts

- Coolant Recovery Reservoir

0.6 liters

0.63 quarts

- Total

4.6 liters

4.9 quarts

Engine Oil (1.0L & 1.3L)

- With Filter Change

3.3 liters

3.5 quarts

- Without Filter Change

3.1 liters

3.3 quarts

Fuel System

- Fuel Tank

40.0 liters

10.6 gallons