For 1990-2009 cars

Condition | Possible Cause
--- | ---
Vehicle does not move in any range (Forward or Reverse) |

• | Low or no fluid

• | Shift cable out of adjustment, binding or damaged

• | Parking lock pawl mechanism locked or frozen

• | Broken torque converter to flywheel bolts

• | Torque converter stator one-way clutch no holding

• | Torque converter failure

• | Valve body spacer plate or gaskets improper position or damaged

• | Check balls omitted or improper position

• | Manual valve binding or sticking

• | Manual valve link disconnected

• | Incorrect line pressure