For 1990-2009 cars

#### Transaxle Range Switch

Connector Part Information |

• | 12089203

• | GRY

Pin | Wire Color | Function
--- | --- | ---
1 | RED | R Position Signal
2 | GRN/RED | D Position Signal
3 | GRN | 2 Position Signal
4 | GRN/BLU | L Position Signal
5 | BLK/YEL | TR Switch Input/Starter Solenoid
6 | BLK/RED | Ign. Start
7 | -- | Not Used
8 | YEL | BACK Fuse
9 | ORN/BLK | P Position Signal
10 | ORN/YEL | N Position Signal