For 1990-2009 cars

## Quarter Upper Trim Panel Replacement Notchback

### Removal Procedure

1. Remove the seat belt from the rear quarter upper trim panel.
2. Remove the rear quarter upper trim panel.

### Installation Procedure

1. Install the rear quarter upper trim panel.
2. Install the seat belt from the rear quarter upper trim panel.

## Quarter Upper Trim Panel Replacement 5 Door Hatchback

### Removal Procedure

1. Remove the seat belt from the rear quarter upper trim panel.
2. Remove the rear rocker trim panel.

Refer to Rear Side Door Sill Plate Replacement

3. Remove the rear quarter upper trim panel.

### Installation Procedure

1. Install the rear quarter upper trim panel.
2. Install the rear rocker trim panel.

Refer to Rear Side Door Sill Plate Replacement .

3. Install the seat belt from the rear quarter upper trim panel.