For 1990-2009 cars

## Engine Controls Connector End Views Notchback

Table 1: | Camshaft Position (CMP) Sensor
Table 2: | Crankshaft Position Sensor (CKP) Sensor
Table 3: | Engine Coolant Temperature (ECT) Sensor
Table 4: | Evaporative Emissions (EVAP) Canister Purge Solenoid Valve
Table 5: | Fuel Injector 1
Table 6: | Fuel Injector 2
Table 7: | Fuel Injector 3
Table 8: | Fuel Injector 4
Table 9: | Fuel Pump/Sender
Table 10: | Oxygen (O2) Sensor (NNB)
Table 11: | Oxygen (O2) Sensor (NNP)
Table 12: | Idle Air Control (IAC) Valve
Table 13: | Ignition Coil (IC) Module
Table 14: | Intake Air Temperature (IAT) Sensor
Table 15: | Knock Sensor (KS)
Table 16: | Manifold Absolute Pressure (MAP) Sensor
Table 17: | Octane Selector Switch
Table 18: | Throttle Position (TP) Sensor

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | 85205-1

• | 3-Way F JR Power Timer 3P Housing Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/BK | -- | Camshaft Position (CMP) Sensor Signal
2 | OG | -- | Low Reference
3 | PK | -- | Ignition 1 Voltage

#### Crankshaft Position Sensor (CKP) Sensor

Connector Part Information |

• | 85205-1

• | 3-Way F JR Power Timer 3P Housing Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU/WH | -- | Crankshaft Position (CKP) Sensor Signal
2 | YE/BK | -- | Low Reference
3 | BK | -- | Ground

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | 12040753

• | 2-Way F Metri-Pack 150 Series Sealed, Pull To Seat (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | YE | -- | Engine Coolant Temperature (ECT) Sensor Signal
B | BN | -- | Low Reference

#### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve

Connector Part Information |

• | 12052643 or AK32229

• | 2-Way F Metri-Pack 150 Series Sealed (RD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-GN | -- | EVAP Canister Purge Valve Solenoid Control
B | PK | -- | Ignition 1 Voltage

#### Fuel Injector 1

Connector Part Information |

• | 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | L-BU/WH | -- | Fuel Injector 1 Control

#### Fuel Injector 2

Connector Part Information |

• | 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | PK/BK | -- | Fuel Injector 2 Control

#### Fuel Injector 3

Connector Part Information |

• | 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | L-GN/BK | -- | Fuel Injector 3 Control

#### Fuel Injector 4

Connector Part Information |

• | 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | BN | -- | Fuel Injector 4 Control

#### Fuel Pump/Sender

Connector Part Information |

• | 36159-1

• | 6-Way F Fuel Pump 6 POS Connector Assembly (BN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Fuel Level Sensor Signal
2 | BK | -- | Ground
3 | BN | -- | Fuel Pump Supply Voltage
4 | PK | -- | Ignition Voltage
5 | YE | -- | Low Fuel Indicator Control
6 | L-BU | -- | Low Reference

#### Oxygen (O2) Sensor (NNB)

Connector Part Information |

• | 12010501

• | 2-Way F Weather Pack Tower, Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | 1665 | Low Reference
B | D-GN/WH | 412 | Heated Oxygen Sensor (HO2S) 1 Signal

#### Oxygen (O2) Sensor (NNP)

Connector Part Information |

• | 12010501

• | 2-Way F Econoseal J-Mark II Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 1665 | Low Reference
2 | D-GN/WH | 412 | Heated Oxygen Sensor (HO2S) 1 Signal

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | PED 12040754

• | 4-Way Metri-Pack 150 Series (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU/BU | -- | Idle Air Control (IAC) B Low Control
B | D-BU | -- | Idle Air Control (IAC) B High Control
C | L-GN/BK | -- | Idle Air Control (IAC) A Low Control
D | D-GN | -- | Idle Air Control (IAC) A High Control

#### Ignition Coil (IC) Module

Connector Part Information |

• | PED 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | -- | Ignition Coil (IC) Timing Control 2 and 3
B | PK | -- | Ignition 1 Voltage
C | OG | -- | Ignition Coil (IC) Timing Control 1 and 4

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | AMP 85202-1

• | 2-Way JR Power Timer 2P Housing Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Intake Air Temperature (IAT) Sensor Signal
2 | BN | -- | Low Reference

#### Knock Sensor (KS)

Connector Part Information |

• | AMP 368215-1

• | 3-Way JPT 3P Assembly for Knock Sensor (GY)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | -- | Knock Sensor (KS) Signal
2 | BN | -- | Low Reference
3 | BN | -- | Low Reference

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | PED 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-BU | -- | Low Reference
B | L-GN | -- | Manifold Absolute Pressure Sensor Signal
C | PU | -- | 5-Volt Reference

#### Octane Selector Switch

Connector Part Information |

• | KET MG 620395

• | 3-Way M Series Sealed (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | -- | Octane Selection Signal 1
2 | BK | -- | Ground
3 | D-GN | -- | Octane Selection Signal 2

#### Throttle Position (TP) Sensor

Connector Part Information |

• | PED 12078090

• | 3-Way F Metri-Pack 150 Series (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | -- | Low Reference
B | PK | -- | 5-Volt Reference
C | L-BU | -- | Throttle Position (TP) Sensor Signal

## Engine Controls Connector End Views Hatchback

Table 1: | Camshaft Position (CMP) Sensor
Table 2: | Crankshaft Position (CKP) Sensor
Table 3: | Engine Coolant Temperature (ECT) Sensor
Table 4: | Evaporative Emissions (EVAP) Canister Purge Solenoid Valve
Table 5: | Fuel Injector 1
Table 6: | Fuel Injector 2
Table 7: | Fuel Injector 3
Table 8: | Fuel Injector 4
Table 9: | Fuel Pump/Sender
Table 10: | Idle Air Control (IAC) Valve
Table 11: | Ignition Coil (IC) Module
Table 12: | Intake Air Temperature (IAT) Sensor
Table 13: | Knock Sensor (KS)
Table 14: | Manifold Absolute Pressure (MAP) Sensor
Table 15: | Octane Selection Switch
Table 16: | Oxygen (O2) Sensor
Table 17: | Throttle Position (TP) Sensor

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | AMP 85205-1

• | 3-Way JR Power Timer 3P Housing Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/BK | 1748 | Camshaft Position (CMP) Sensor Signal
2 | L-BU | 52 | Camshaft Position (CMP) Sensor Return
3 | BN | 1733 | Ignition 1 Voltage

#### Crankshaft Position (CKP) Sensor

Connector Part Information |

• | AMP 85205-1

• | 3-Way JR Power Timer 3P Housing Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU/WH | 1869 | Low Reference
2 | YE/BK | 1868 | Crankshaft Position (CKP) Sensor Signal
3 | BK/WH | 51 | Ground

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | PED 12040753

• | 2-Way F Metri-Pack 150 Series Sealed, Pull To Seat (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-GN | 410 | Engine Coolant Temperature (ECT) Sensor Signal
B | GN | 808 | Low Reference

#### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve

Connector Part Information |

• | PED 12052643

• | 2-Way F Metri-Pack 150 Series Sealed (RD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | 452 | EVAP Canister Purge Solenoid Control
B | BN | 1733 | Ignition 1 Voltage

#### Fuel Injector 1

Connector Part Information |

• | AMP 368468-1

• | 2-Way Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 1733 | Ignition 1 Voltage
2 | BN/BK | 1747 | Fuel Injector 1 Control

#### Fuel Injector 2

Connector Part Information |

• | AMP 368468-1

• | 2-Way Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 1733 | Ignition 1 Voltage
2 | L-GN | 1746 | Fuel Injector 2 Control

#### Fuel Injector 3

Connector Part Information |

• | AMP 368468-1

• | 2-Way Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 1733 | Ignition 1 Voltage
2 | BN/WH | 1745 | Fuel Injector 3 Control

#### Fuel Injector 4

Connector Part Information |

• | AMP 368468-1

• | 2-Way Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 1733 | Ignition 1 Voltage
2 | YE | 1744 | Fuel Injector 4 Control

#### Fuel Pump/Sender

Connector Part Information |

• | AMP 936159-1

• | 6-Way FUEL PUMP 6POS Connector Assembly (BN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 1936 | Fuel Level Sensor Signal
2 | BK | 850 | Ground
3 | BN | 1723 | Fuel Pump Supply Voltage
4 | BK | 850 | Ground
5 | PU | 172 | Low Fuel Indicator Control
6 | L-BU | 1937 | Low Reference

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | PED 12040754

• | 4-Way F Metri-Pack 150 Series (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-GN | 415 | Idle Air Control (IAC) B Low Control
B | L-GN | 417 | Idle Air Control (IAC) B High Control
C | WH/D-BU | 533 | Idle Air Control (IAC) A Low Control
D | L-GN | 534 | Idle Air Control (IAC) A High Control

#### Ignition Coil (IC) Module

Connector Part Information |

• | PED 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | OG | 423 | Ignition Coil (IC) 2 and 3 Control
B | PK | 539 | Ignition 1 Voltage
C | WH | 406 | Ignition Coil (IC) 1 and 4 Control

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | AMP 85202-1

• | 2-Way JR Power Timer 2P Housing Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 468 | Intake Air Temperature (IAT) Sensor Signal
2 | D-GN | 808 | Low Reference

#### Knock Sensor (KS)

Connector Part Information |

• | AMP 368215-1

• | 3-Way F JPT 3P Assembly for Knock Sensor (GY)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/BK | 496 | Knock Sensor (KS)
2 | D-BU/WH | 1876 | Low Reference
3 | D-GN | 808 | Low Reference

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | PED 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | 433 | Low Reference
B | L-BU | 432 | Manifold Absolute (MAP) Pressure Sensor Signal
C | YE/BK | 469 | 5-Volt Reference

#### Octane Selection Switch

Connector Part Information |

• | KET MG 620395

• | 3-Way M (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 892 | Octane Selection Switch
2 | BK/WH | 51 | Ground
3 | PU | 890 | Octane Selection Switch

#### Oxygen (O2) Sensor

Connector Part Information |

• | PED 12010501

• | 2-Way F Weather Pack Tower Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | 428 | Oxygen (O2) Sensor Signal
B | D-BU/BK | 429 | Oxygen (O2) Sensor Low Reference

#### Throttle Position (TP) Sensor

Connector Part Information |

• | PED 12078090

• | 3-Way F Metri-Pack 150 Series (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 427 | 5-Volt Reference
B | D-BU | 426 | Low Reference
C | WH | 425 | Throttle Position (TP) Sensor Signal