For 1990-2009 cars

Figure 1: |

#### Airbag Harness Routing (RHD Shown, LHD Similar)

(1) | Inflatable Restraint Side Impact Sensor - Right
(2) | Seat Belt Pretensioner - Right
(3) | Inflatable Restraint Side Impact Module - Right
(4) | Inflatable Restraint Sensing and Diagnostic Module (SDM)
(5) | Passenger Pressence System (PPS) Sensor
(6) | Inflatable Restraint Side Impact Module - Left
(7) | Seat Belt Pretensioner - Left
(8) | Infltable Restraint Side Impact Sensor - Left
(9) | Passenger Airbag Disable Switch
(10) | Glove Box Switch
(11) | Inflatable Restraint - I/P Module
(12) | X216
(13) | Inflatable Restraint Steering Wheel Module
(14) | G203

Figure 2: |

#### Engine Harness Routing (1.2L)

(1) | Battery
(2) | Camshaft Position (CMP) Sensor
(3) | Heated Oxygen Sensor (HO2S) 2
(4) | Heated Oxygen Sensor (HO2S) 1
(5) | Ignition Coil Module
(6) | X106
(7) | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
(8) | A/C Refrigerant Pressure Sensor
(9) | Power Steering Pressure Switch
(10) | Oil Pressure Switch
(11) | Generator
(12) | G104
(13) | Starter
(14) | Knock Sensor (KS)
(15) | Crankshaft Position (CKP) Sensor
(16) | Engine Coolant Temperature (ECT) Sensor
(17) | Exhaust Gas Recirculation (EGR) Vavle
(18) | X206
(19) | X204
(20) | Octane Selection Switch
(21) | G103
(22) | Fuse Block - Underhood
(23) | Engine Control Module (ECM)

Figure 3: |

#### Engine Harness Routing (1.4L/1.6L)

(1) | Fuse Block - Underhood X1
(2) | Crankshaft Position (CKP) Sensor
(3) | Backup Switch (D16/Y4M)
(4) | Heated Oxygen Sensor (HO2S) 1
(5) | Ignition Coil Module
(6) | Exhaust Gas Recirculation (EGR) Valve
(7) | Fuel Injector 1
(8) | Manifold Absolute Pressure (MAP) Sensor
(9) | Fuel Injector 2
(10) | Fuel Injector 3
(11) | Fuel Injector 4
(12) | Camshaft (CMP) Sensor
(13) | Intake Air Temperature (IAT) Sensor
(14) | A/C Refrigerant Pressure Sensor
(15) | Throttle Position (TP) Sensor
(16) | Idel Air Control (IAC) Valve
(17) | Generator
(18) | Engine Coolant Temperature (ECT) Sensor
(19) | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
(20) | Oil Pressure Switch
(21) | Knock Sensor (KS)
(22) | VGI Solenoid Valve
(23) | Starter
(24) | G104
(25) | Vehicle Speed Sensor (VSS) (D16/Y4M)
(26) | X105
(27) | Octane Selector Switch
(28) | Rough Road Sensor
(29) | X204
(30) | G103
(31) | Engine Control Module (ECM) X2
(32) | Engine Control Module (ECM) X1

Figure 4: |

#### Engine Harness Routing (1.5L)

(1) | Fuse Block - Underhood
(2) | X101
(3) | Battery
(4) | Ignition Coil Module
(5) | Manifold Absolute Pressure (MAP) Sensor
(6) | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
(7) | Engine Coolant Temperature (ECT) Sensor
(8) | Backup Switch (D16/Y4M)
(9) | Crankshaft Position (CKP) Sensor
(10) | Fuel Injector 1
(11) | Fuel Injector 2
(12) | Fuel Injector 3
(13) | Fuel Injector 4
(14) | Camshaft Position (CMP) Sensor
(15) | Heated Oxygen Sensor (HO2S) 1
(16) | Intake Air Temperature (IAT) Sensor
(17) | A/C Refridgerant Pressure Sensor
(18) | Oil Pressure Switch
(19) | Throttle Position (TP) Sensor
(20) | Idle Air Control (IAC) Valve
(21) | Generator
(22) | Knock Sensor (KS)
(23) | Starter
(24) | G104
(25) | Vehicle Speed Sensor (VSS) (D16/Y4M)
(26) | X105
(27) | Octane Selector Switch
(28) | X204
(29) | G103
(30) | Engine Control Module X1
(31) | Engine Control Module X2

Figure 5: |

#### Floor Harness Routing

(1) | Speaker - Left Rear
(2) | X402
(3) | X401
(4) | Rear Compartment Lamp
(5) | Door Jamb Switch - Left Rear
(6) | Wheel Speed Sensor (WSS) - Left Rear
(7) | X371
(8) | Door Jamb Switch - Driver
(9) | X351
(10) | X211
(11) | X213
(12) | X212
(13) | X214
(14) | X361
(15) | Seat Belt Switch - Driver
(16) | Park Brake Switch
(17) | Auxiliary Power Outlet
(18) | Door Jamb Switch - Passenger
(19) | X381
(20) | Fuel Pump and Sender Assembly
(21) | Wheel Speed Sensor - Right Rear
(22) | Door Jamb Switch - Right Rear
(23) | G403
(24) | Tail Lamp - Right
(25) | Speaker - Right Rear
(26) | G401
(27) | Tail Lamp - Left

Figure 6: |

#### Front Harness Routing

(1) | X208
(2) | Windshield Wiper Motor
(3) | Turn Signal Repeater - Left
(4) | Brake Fluid Level Switch
(5) | Wheel Speed Sensor (WSS) - Left Front
(6) | Electronic Brake Control Module (EBCM)
(7) | X102
(8) | X103
(9) | Fuse Block - Underhood
(10) | Inflatable Restraint Front Discriminating Sensor - Left
(11) | Park/Turn Signal Lamp - Left Front
(12) | Headlamp - Left
(13) | Position Lamp/Headlamp Leveling Actuator - Left
(14) | G102
(15) | Hood Ajar Switch
(16) | Windshield Washer Fluid Pump (Notchback)/Windshield Washer Fluid Pump - Front (Hatchback)
(17) | Horn
(18) | Ambient Air Temperature Sensor
(19) | Fog Lamp - Left Front
(20) | Cooling Fan
(21) | Position Lamp/Headlamp Leveling Actuator - Right
(22) | Heated Oxygen Sensor (HO2S) 2
(23) | A/C Compressor Clutch
(24) | Fog Lamp - Right Front
(25) | G101
(26) | Headlamp - Right
(27) | Inflatable Restraint Front Discriminating Sensor - Right
(28) | Park/Turn Signal Lamp - Right Front
(29) | Wheel Speed Sensor (WSS) - Right Front
(30) | Turn Signal Repeater - Right

Figure 7: |

#### Instrument Panel Harness Routing (LHD Shown, RHD Similar)

(1) | G201
(2) | BLINK Relay
(3) | Inflatable Restraint Steering Wheel Module Coil
(4) | Stop Lamp Switch
(5) | Radio X1
(6) | Radio X2
(7) | Clock
(8) | Air Temperature Actuator
(9) | X217
(10) | Blower Motor Resistor
(11) | Blower Motor
(12) | Radio Antenna
(13) | HVAC Control Module
(14) | X215
(15) | Cigar Lighter
(16) | G203
(17) | PRNDL Lamp
(18) | Shift Program Switch (MLQ)
(19) | Automatic Transmission Shift Lever (MLQ)
(20) | Hazard Switch
(21) | Blower Motor Switch
(22) | Data Link Connector (DLC)
(23) | Fuse Block - I/P
(24) | Folding Mirror Unit
(25) | Fuse Block - I/P X1
(26) | I/P Dimmer Switch
(27) | PARK/NEUTRAL POSITION (PNP) Relay
(28) | Outside Rearview Mirror Switch

Figure 8: |

#### Rear Harness Routing

(1) | Tail Lamp - Right
(2) | G402
(3) | Tail Lamp - Left
(4) | X401