For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
5th/Reverse Gear Shift Shaft Bolt | 13 N·m | 10 lb ft
Back Up Light Switch Nut | 17 N·m | 13 lb ft
Counter Shaft 5th Gear Nut | 70 N·m | 52 lb ft
Crankshaft Position Sensor Bolt | 7 N·m | 62 lb in
Differential Ring Gear Bolt | 90 N·m | 66 lb ft
Engine Mounting Rear Damping Bolts | 55 N·m | 41 lb ft
Front Exhaust Pipe Nut - Exhaust Manifold Side/Muffler Side | 30 N·m | 22 lb ft
Gear Shift Lever Bolts | 6 N·m | 53 lb in
Ground Wire Bolt | 13 N·m | 10 lb ft
High Speed Shift Shaft Bolt - 5th Gear Shift | 13 N·m | 10 lb ft
Low Speed Shift Shaft Bolt - 3rd and 4th Gear Shift | 13 N·m | 10 lb ft
Oil Drain Plug | 28 N·m | 21 lb ft
Oil Level Plug | 28 N·m | 21 lb ft
Radiator Lower Hose Bracket Bolts | 12 N·m | 106 lb in
Rear Damping Block Connection Nut and Bolt | 82 N·m | 61 lb ft
Reverse Idle Gear Shaft Bolt | 23 N·m | 17 lb ft
Reverse Shift Lever Bolt | 23 N·m | 17 lb ft
Select Cable Nut - Shift Lever Side | 10 N·m | 89 lb in
Side Cover - Clutch Plate | 10 N·m | 89 lb in
Side Cover Bolt | 10 N·m | 89 lb in
Side Cover Plate Bolt | 7 N·m | 62 lb in
Shift Interlock Bolt | 23 N·m | 17 lb ft
Speedometer Driven Gear Bolt | 7 N·m | 62 lb in
Transaxle Lower Bolt | 60 N·m | 44 lb ft
Transaxle Mounting Bolt - Rear Bracket | 50 N·m | 37 lb ft
Transaxle Mounting Bolts - Rear Damping Block | 55 N·m | 41 lb ft
Transaxle Upper Bolt - Engine Side | 60 N·m | 44 lb ft