For 1990-2009 cars

The fuel filler door attaches to the fuel tank pocket on the right side of the vehicle.

### Rear Deck Lid (Notchback)

The rear deck lid consists of an inner and an outer panel hemmed around the perimeter and bonded together with structural adhesive. The torque rods assist in the opening of the rear deck lid and hold it in the open position.

### Hatchback Door

The hatchback door consists of the rear hatch glass within a steel frame. The steel frame is made of an inner and an outer panel hemmed around the perimeter, and bonded together with structural adhesive. The gas support assemblies assist in the opening of the hatchback door, and can hold the door open.