For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Overall Length

- Four Door

4 310 mm

169.7 in

- Five Door

3 880 mm

152.6 in

Overhang - Front

- Four Door

833 mm

32.8 in

- Five Door

813 mm

32.0 in

Overhang - Rear

- Four Door

997 mm

39.5 in

- Five Door

587 mm

23.1 in

Overall Width Four Door | 1 710 mm | 69.3 in
Overall Width Five Door | 1 670 mm | 65.7 in
Overall Height Four Door | 1 505 mm | 59.3 in
Overall Height Five Door | 1 495 mm | 58.9 in
Minimum Ground Clearance Four Door | 155 mm | 6.1 in
Minimum Ground Clearance Five Door | 150 mm | 5.9 in
Wheel Base | 2 480 mm | 97.6 in
Tread
Front | 1 450 mm | 57.1 in
Rear Four Door | 1 430 mm | 56.3 in
Rear Five Door | 1 410 mm | 55.1 in

#### Vehicle Weights - Four Door

Application | Specification
--- | ---
Metric | English
Manual

- Curb Weight - Standard

1 010 kg

2 227 lb

- Curb Weight - Optional

1 065 kg

2 348 lb

- Gross Vehicle Weight

1 505 kg

3 318 lb

Automatic
Curb Weight - Standard | 1 015 kg | 2 237 lb
Curb Weight - Optional | 1 070 kg | 2 358 lb

- Gross Vehicle Weight

1 510 kg

3 329 lb

Passenger Capacity | 5

#### Vehicle Weights - Five Door

Application | Specification
--- | ---
Metric | English
Manual

- Curb Weight - Standard

1 000 kg

2 205 lb

- Curb Weight - Optional

1 055 kg

2 326 lb

- Gross Vehicle Weight

1 505 kg

3 318 lb

Automatic
Curb Weight - Standard | 1 005 kg | 2 216 lb
Curb Weight - Optional | 1 060 kg | 2 237 lb

- Gross Vehicle Weight

1 510 kg

3 329 lb

Passenger Capacity | 5