For 1990-2009 cars

## Speedometer Replacement Hatchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster. Refer to Instrument Cluster Replacement .
3. Remove the instrument cluster lens and the face plate.
4. Remove the screws and the speedometer from the instrument cluster.

### Installation Procedure

1. Install the speedometer to the instrument cluster with the screws.
2. Install the instrument cluster lens and the face plate.
3. Install the instrument cluster. Refer to Instrument Cluster Replacement .
4. Connect the negative battery cable.