For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Hose Inlet Fitting-to-Caliper Bolt | 40 N·m | 30 lb ft
Caliper Bleeder Valve | 6 N·m | 53 lb in
Caliper-to-Steering Knuckle Mounting Bolts | 95 N·m | 70 lb ft
Retaining Frame-to-Caliper Housing Bolts | 27 N·m | 20 lb ft
Rotor-to-Front Wheel Hub Detent Screw | 4 N·m | 35 lb in
Splash Shield-to-Steering Knuckle Screws | 4 N·m | 35 lb in