For 1990-2009 cars

Figure 1: |

#### HVAC Blower Controls

(1) | Recirculation Actuator
(2) | Blower Motor Resistor
(3) | Blower Motor
(4) | HVAC Control and Blower Switch

Figure 2: |

#### A/C Compressor

(1) | A/C Compressor Clutch
(2) | A/C Refrigerent Pressure Sensor

Figure 3: |

#### V5 Compressor Assembly

(1) | Shaft Nut
(2) | Compressor Shaft
(3) | Shaft and Guide Pin Assembly Cylinder
(4) | Rear Head O-Ring
(5) | Suction Reed
(6) | Valve Plate
(7) | Rear Head Gasket
(8) | Retaining Ring
(9) | Control Valve O-Ring
(10) | Compressor Control Valve
(11) | Rear Head Compressor
(12) | Adaptor Compressor
(13) | Pressure Relief Valve O-Ring
(14) | Pressure Relief Valve
(15) | Adaptor Bolt
(16) | Through-Bolt
(17) | Clutch Hub Key
(18) | Clutch and Hub Keyway
(19) | Through-Gasket
(20) | Oil Drain Plug
(21) | Bearing
(22) | Compressor Housing-to-Cylinder O-Ring
(23) | Race
(24) | Thrust Washer
(25) | Compressor Housing
(26) | Shaft Seal O-Ring
(27) | Shaft Lip Seal
(28) | Seal Retaining Ring
(29) | Clutch Coil
(30) | Rotor Pulley
(31) | Pulley Bearing
(32) | Pulley Bearing-to-Head Retaining Ring
(33) | Drive Plate Clutch

Figure 4: |

#### SP10 Compressor Assembly (1.2L Engine)

(1) | Shaft Bolt
(2) | Shaft Bolt Washer
(3) | Clutch and Drive Assembly
(4) | Air Gap Shim
(5) | Retaining Ring
(6) | Pulley and Bearing Assembly
(7) | Retaining Ring
(8) | Coil and Housing Assembly
(9) | Through Bolt
(10) | Retaining Ring
(11) | Lip Seal Assembly
(12) | Front Head
(13) | Front Head Gasket
(14) | Discharge Reed Retainer
(15) | Discharge Reed
(16) | Front Valve Plate
(17) | Suction Reed
(18) | Parallel Locating Pin
(19) | Front Compressor Cylinder
(20) | Swash Plate and Shaft Assembly
(21) | Piston Shoe
(22) | Piston Assembly
(23) | Thrust Bearing
(24) | Thrust Bearing
(25) | Cylinder O-Ring
(26) | Bushing
(27) | Roll Locating Pin
(28) | Rear Compressor Cylinder
(29) | Main Shaft Bearing
(30) | Rear Valve Plate
(31) | Rear Head Gasket
(32) | Rear Head